* WARNNING *
	Updating R1.x to R2.x will CRASH SYSTEM BIOS,
	    where 'x' represents any number of version.
	DO NOT UPDATE R1.x to R2.x with go.nsh.
	Contact AAEON if you need to update from R1.x to R2.x

Note:	If you are already with R2.x BIOS, you are good to update to newer version with go.nsh.

Note:	before start, remove all bootable devices like SATA HDD.
	Otherwise you may need to change to different drive label (fs1, fs2...etc) instead of fs0: in step 3

1. Put BIOS in USB drive
2. Select boot for Built-in Shell (or shell loader in USB drive if present).
3. Move operating directory to USB drive (fs0 or other labels)
   > fs0:
4. Enter the directory with BIOS file and update batch
5. Execute update batch (Go.nsh)
6. Confirm update procedure is passed without problem
7. When BIOS flash finished, the system will reboot automatically.