
Note:	
	If update BIOS from "K236AM15 or below" to "K236AM16 or above", please update both BIOS and SPS F/W.
	Otherwise, please update BIOS only.

Update BIOS (Go.nsh):
	1. Copy BIOS upgrade folder into the UEFI Shell bootable USB Flash Drive, and plug the USB Flash Drive to the system.
	2. Enter the system BIOS Setup, select the UEFI Shell bootable USB Flash Drive as "Boot Option #1" .
	3. After the system boots to the UEFI Shell, switch to the BIOS upgrade folder.
	4. Execute update batch "Go.nsh" .
	5. After the upgrade is completed, the system will automatically reset and BIOS updated successfully. 

Optional:
Update SPS F/W (GO_SPS.nsh):
	1. Before SPS F/W Update, BIOS update should be done first.
	2. Copy BIOS upgrade folder into the UEFI Shell bootable USB Flash Drive, and plug the USB Flash Drive to the system.
	3. Enter the system BIOS Setup,  
	   enable the IntelRCSetup -> "Relax Security Configuration" item,
	   and select the UEFI Shell bootable USB Flash Drive as "Boot Option #1" .
	4. After the system boots to the UEFI Shell, switch to the BIOS upgrade folder.
	5. Execute update batch "GO_SPS.nsh" .
	6. After the upgrade is completed, the system will automatically reset and SPS F/W updated successfully. 
	

