
Except the following cases need to upgrade BIOS and SPS F/W, otherwise please upgrade the BIOS only.
(1) Upgrade BIOS from "K860BM11 or below" to "K860BM12 or above".


Upgrade BIOS Only :
	1. Copy BIOS upgrade folder into the UEFI Shell bootable USB Flash Drive, and plug the USB Flash Drive to the system.
	2. Enter the system BIOS Setup, select the UEFI Shell bootable USB Flash Drive as "Boot Option #1" then Save Changes & Reset.
	3. After the system boots to the UEFI Shell, switch to the BIOS upgrade folder.
	4. Execute upgrade batch "GO.nsh" .
	5. After the upgrade is completed, please cut off the AC power to have the changes take effect.


Upgrade SPS F/W (Optional) :
	1. Please use a jumper to short the CN31 pin connector.
	2. Copy BIOS upgrade folder into the UEFI Shell bootable USB Flash Drive, and plug the USB Flash Drive to the system.
	3. Enter the system BIOS Setup, select the UEFI Shell bootable USB Flash Drive as "Boot Option #1" then Save Changes & Reset.
	4. After the system boots to the UEFI Shell, switch to the BIOS upgrade folder.
	5. Execute update batch "GO_SPS.nsh" .
	6. After the upgrade is completed, please cut off the AC power to have the changes take effect.
	7. Please remember to remove the jumper after SPS F/W upgrade completed.

