@echo ^ ""

@echo ^******************* !! Note !! *******************
@echo ^Intel Management Engine F/W needs to be upgraded, please follow 

@echo ^the steps below :

@echo ^ ""

@echo ^1. Enter `q` to quit.

@echo ^2. Reboot the system.

@echo ^3. Enter BIOS setup menu and switch to 'Firmware Update Configuration' 

@echo ^   under Advanced.

@echo ^4. Change BIOS setup option 'Me FW Image Re-Flash' to 'Enabled'.

@echo ^5. Save Changes and Reset.

@echo ^6. Boot to EFI Shell directly and execute go.nsh.

@echo ^7. Press any keys to continue.

@echo ^8. Flash progress will begin.

@echo ^ ""

@echo ^* Note:

@echo ^* 'Me FW Image Re-Flash' will be reset to 'Disabled' after every system reboot.

@echo ^***********************************************

pause

AfuEfix64_5.15.03.0081.efi UXRPAM18.bin /P /N /B /ME /RLC:M
