Applied Values (+Defaults) Report 

  
 HE 104 PWBA <MIL-217F-2 P. stress>  
 Assembly Ref.Des.: A1A1H1,   IC-Analog
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	         
  Type   	                       
 Application(GaAs MMIC)	       # of      
     transist.   	Active
 pins 	          
  Package 	 Years in 
production	        
  Qual  	 Theta 
 jc/ja 	 Power    
 dissipat.	       
 Tc/Ta 	       
  Tj   	
1.7.36	IC1	LTC1159CS-5	 Linear	 ---	  >100 to 300	16	 DIP Nonh	      2.0	 Commerc	   ---	      ---	  32.0	  37.0	              
1.7.37	1C2	LTC1266CS	 Linear	 ---	  >100 to 300	16	 DIP Nonh	      2.0	 Commerc	   ---	      ---	  32.0	  37.0	              
1.7.38	Q6	RECTIFIER	 Linear	 ---	     1 to 100	3	 DIP Nonh	      2.0	 Commerc	   ---	      ---	  32.0	  37.0	              

 Assembly Ref.Des.: A1A1H1,   Resistor
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	       
 Style 	        
  PSR   	        
 Poper  	       
  DT   	                  
       Qual       	
1.7.16	R3-6,..,25	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.17	R13,22	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.18	R15	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.19	R19	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.20	R1,14	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.21	R11,27	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.22	R12,20	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.23	R2,8	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.24	R16,23	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.26	R10	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.27	R26	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.28	R18	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.29	R9	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.30	R7	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.31	R23A,23B	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        

 Assembly Ref.Des.: A1A1H1,   Potentiometer
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	       
 Style 	        
  PSR   	       
  DT   	                  
       Qual       	
1.7.15	R21	RESISTOR	 RV	   0.20	   1.0	 Non-Established	       

 Assembly Ref.Des.: A1A1H1,   Capacitor
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	       
 Style 	             
 Capacitance 	      
 VSR  	 Circuit resist. 
  (CSR & CWR)    	       
  DT   	                  
       Qual       	
1.7.1	C4, C21	CAPACITOR	 CDR	 4.7E-002 uF	 0.20	             ---	   0.0	 M	         
1.7.2	C8,10,19	CAPACITOR	 CDR	    0.100 uF	 0.20	             ---	   0.0	 M	         
1.7.3	C6,17	CAPACITOR	 CDR	 1000.000 pF	 0.20	             ---	   0.0	 M	         
1.7.4	C23	CAPACITOR	 CDR	  100.000 pF	 0.20	             ---	   0.0	 M	         
1.7.5	C9,13,..16	CAPACITOR	 CE	  402.200 uF	 0.20	             ---	   1.0	 Non-Established	         
1.7.6	C5	CAPACITOR	 CDR	  200.000 pF	 0.20	             ---	   0.0	 M	         
1.7.7	C18,24	CAPACITOR	 CDR	    1.000 uF	 0.20	             ---	   0.0	 M	         
1.7.8	C8A-C8D	CAPACITOR	 CE	  402.200 uF	 0.20	             ---	   1.0	 Non-Established	         
1.7.9	C20,22,27	CAPACITOR	 CDR	  330.000 pF	 0.20	             ---	   0.0	 M	         
1.7.10	C25	CAPACITOR	 CWR	    4.700 uF	 0.20	          0.1000	   0.0	 M	         
1.7.11	C1,7,12	CAPACITOR	 CWR	    4.000 uF	 0.20	          0.1000	   0.0	 M	         
1.7.12	C9B,C9C	CAPACITOR	 CE	  402.200 uF	 0.20	             ---	   1.0	 Non-Established	         
1.7.13	C11	CAPACITOR	 CDR	  100.000 pF	 0.20	             ---	   0.0	 M	         
1.7.14	C14	CAPACITOR	 CWR	    1.000 uF	 0.20	          0.1000	   0.0	 M	         
1.7.25	C2,3	CAPACITOR	 CE	  402.200 uF	 0.20	             ---	   1.0	 Non-Established	         

 Assembly Ref.Des.: A1A1H1,   LF Diode
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	             
    Style    	     
 VSR 	                
  Application   	              
 Construction 	  Forward  
 current(A)	         
  Qual   	 Theta 
 jc/ja 	 Power    
 dissipat.	       
 Tc/Ta 	       
  Tj   	
1.7.34	D4,7	DIODE	 DIODE_SI	 0.2	 Voltage Refere	 Non-metallur	       ---	 LOWER	   ---	      ---	  32.0	  33.0	             

 Assembly Ref.Des.: A1A1H1,   LF Transistor
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	             
    Style    	     
 VSR 	                
  Application   	  Power    
  rated    	         
  Qual   	 Theta 
 jc/ja 	 Power    
 dissipat.	       
 Tc/Ta 	       
  Tj   	
1.7.39	Q3	P CHANNEL JFET	 FET_SI_JFET	 ---	 Linear	     1.000	 LOWER	   ---	      ---	  32.0	  33.0	            
1.7.40	Q2	NPN TRANSISTOR	 NPN_SI	 0.0	 Linear	     1.000	 JAN	   ---	      ---	  32.0	  33.0	            
1.7.41	Q1,8	NPN TRANSISTOR	 NPN_GE	 0.2	 Linear	     1.000	 LOWER	   ---	      ---	  32.0	  33.0	            
1.7.42	Q5	FET	 FET_SI_JFET	 ---	 Switching	     1.000	 LOWER	   ---	      ---	  32.0	  33.0	            
1.7.43	Q4,7	FET	 FET_SI_JFET	 ---	 Switching	     1.000	 JANTX	   ---	      ---	  32.0	  33.0	            

 Assembly Ref.Des.: A1A1H1,   Optoelectronic
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	                                   
                Style              	 # of characters 
    (DISPLAY)    	 Logic exists  
 (DISPLAY)     	         
  Qual   	 Theta 
 jc/ja 	 Power    
 dissipat.	       
 Tc/Ta 	       
  Tj   	
1.7.35	LED1-4	LED	 LED DISCRETE	 ---	 ---	 LOWER	   ---	      ---	  32.0	  52.0	           

 Assembly Ref.Des.: A1A1H1,   Inductive
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	                                
         Family type            	       
  DT   	          
   Qual   	
1.7.32	L2	TOR-50	 Coil,Fixed Inductor or Choke	   5.0	 Lower	      
1.7.33	L3	COIL	 Coil,Fixed Inductor or Choke	   5.0	 Lower	      

 Assembly Ref.Des.: A1A1H1,   PWB
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	            
 Technology 	  # of  
 layers 	          
 WAVE(N1) 	          
 HAND(N2) 	          
   Qual   	
1.7.44	PWB	PWB	 Printed wi	 2	 100	 2	 Lower