Tree Diagram Report 

 Project name: SKIPPER                                      
  
MTBF=164612.13; Qty=1  
1 C4,_C21; MTBF=66333520; Qty=2  
2 C8,10,19; MTBF=61975763; Qty=3  
3 C6,17; MTBF=93804114; Qty=2  
4 C23; MTBF=1.15E+008; Qty=1  
5 C9,13,..16; MTBF=69668716; Qty=5  
6 C5; MTBF=1.08E+008; Qty=1  
7 C18,24; MTBF=50375790; Qty=1  
8 C8A-C8D; MTBF=69668716; Qty=5  
9 C20,22,27; MTBF=1.04E+008; Qty=3  
10 C25; MTBF=5.30E+008; Qty=1  
11 C1,7,12; MTBF=5.50E+008; Qty=3  
12 C9B,C9C; MTBF=69668715; Qty=2  
13 C11; MTBF=1.15E+008; Qty=1  
14 C14; MTBF=7.57E+008; Qty=1  
15 R21; MTBF=14652714; Qty=1  
16 R3-6,..,25; MTBF=7295235.6; Qty=7  
17 R13,22; MTBF=7295235.5; Qty=2  
18 R15; MTBF=7295235.5; Qty=1  
19 R19; MTBF=7295235.5; Qty=1  
20 R1,14; MTBF=7295235.5; Qty=2  
21 R11,27; MTBF=7295235.5; Qty=2  
22 R12,20; MTBF=7295235.5; Qty=2  
23 R2,8; MTBF=7295235.5; Qty=1  
24 R16,23; MTBF=7295235.5; Qty=2  
25 C2,3; MTBF=69668715; Qty=2  
26 R10; MTBF=7295235.5; Qty=1  
27 R26; MTBF=7295235.5; Qty=1  
28 R18; MTBF=7295235.5; Qty=1  
29 R9; MTBF=7295235.5; Qty=1  
30 R7; MTBF=7295235.5; Qty=1  
31 R23A,23B; MTBF=7295235.5; Qty=2  
32 L2; MTBF=1.87E+009; Qty=1  
33 L3; MTBF=1.87E+009; Qty=1  
34 D4,7; MTBF=4265700.4; Qty=2  
35 LED1-4; MTBF=72634831; Qty=1  
36 IC1; MTBF=2933440.8; Qty=1  
37 1C2; MTBF=2933440.8; Qty=1  
38 Q6; MTBF=13548433; Qty=1  
39 Q3; MTBF=2527822.7; Qty=1  
40 Q2; MTBF=7.70E+008; Qty=1  
41 Q1,8; MTBF=1.81E+008; Qty=2  
42 Q5; MTBF=5416762.7; Qty=1  
43 Q4,7; MTBF=29792195; Qty=2  
44 PWB; MTBF=45955883; Qty=1  

       Assembly Composite Report 

 Project name: HE104
  
Assembly Ref.Des.: A1A1H1, ID: 1.7, Description: POWER SUPPLY.  
Environment: NS, Temperature:     25.00 °C, L (xE-6 ): 6.07     , MTBF(hours): 164612.13
                          
 ID                      	                               
 PN                            	           
 RefDes    	    
 Qty	     L   
  xE-6   	 L(K,Qty)
  xE-6   	 Contrib. 
 to NHA[%]	
1.7.1	 CAPACITOR	 C4, C21	  2	 0.01508	 0.03015	     0.50	       
1.7.2	 CAPACITOR	 C8,10,19	  3	 0.01614	 0.04841	     0.80	       
1.7.3	 CAPACITOR	 C6,17	  2	 0.01066	 0.02132	     0.35	       
1.7.4	 CAPACITOR	 C23	  1	 0.008665	 0.008665	     0.14	       
1.7.5	 CAPACITOR	 C9,13,..16	  5	 0.01435	 0.07177	     1.18	       
1.7.6	 CAPACITOR	 C5	  1	 0.009223	 0.009223	     0.15	       
1.7.7	 CAPACITOR	 C18,24	  1	 0.01985	 0.01985	     0.33	       
1.7.8	 CAPACITOR	 C8A-C8D	  5	 0.01435	 0.07177	     1.18	       
1.7.9	 CAPACITOR	 C20,22,27	  3	 0.009648	 0.02894	     0.48	       
1.7.10	 CAPACITOR	 C25	  1	 0.001885	 0.001885	     0.03	       
1.7.11	 CAPACITOR	 C1,7,12	  3	 0.001817	 0.00545	     0.09	       
1.7.12	 CAPACITOR	 C9B,C9C	  2	 0.01435	 0.02871	     0.47	       
1.7.13	 CAPACITOR	 C11	  1	 0.008665	 0.008665	     0.14	       
1.7.14	 CAPACITOR	 C14	  1	 0.001321	 0.001321	     0.02	       
1.7.15	 RESISTOR	 R21	  1	 0.06825	 0.06825	     1.12	       
1.7.16	 RESISTOR	 R3-6,..,25	  7	 0.1371	 0.9595	    15.80	       
1.7.17	 RESISTOR	 R13,22	  2	 0.1371	 0.2742	     4.51	       
1.7.18	 RESISTOR	 R15	  1	 0.1371	 0.1371	     2.26	       
1.7.19	 RESISTOR	 R19	  1	 0.1371	 0.1371	     2.26	       
1.7.20	 RESISTOR	 R1,14	  2	 0.1371	 0.2742	     4.51	       
1.7.21	 RESISTOR	 R11,27	  2	 0.1371	 0.2742	     4.51	       
1.7.22	 RESISTOR	 R12,20	  2	 0.1371	 0.2742	     4.51	       
1.7.23	 RESISTOR	 R2,8	  1	 0.1371	 0.1371	     2.26	       
1.7.24	 RESISTOR	 R16,23	  2	 0.1371	 0.2742	     4.51	       
1.7.25	 CAPACITOR	 C2,3	  2	 0.01435	 0.02871	     0.47	       
1.7.26	 RESISTOR	 R10	  1	 0.1371	 0.1371	     2.26	       
1.7.27	 RESISTOR	 R26	  1	 0.1371	 0.1371	     2.26	       
1.7.28	 RESISTOR	 R18	  1	 0.1371	 0.1371	     2.26	       
1.7.29	 RESISTOR	 R9	  1	 0.1371	 0.1371	     2.26	       
1.7.30	 RESISTOR	 R7	  1	 0.1371	 0.1371	     2.26	       
1.7.31	 RESISTOR	 R23A,23B	  2	 0.1371	 0.2742	     4.51	       
1.7.32	 TOR-50	 L2	  1	 0.0005347	 0.0005347	     0.01	       
1.7.33	 COIL	 L3	  1	 0.0005347	 0.0005347	     0.01	       
1.7.34	 DIODE	 D4,7	  2	 0.2344	 0.4689	     7.72	       
1.7.35	 LED	 LED1-4	  1	 0.01377	 0.01377	     0.23	       
1.7.36	 LTC1159CS-5	 IC1	  1	 0.3409	 0.3409	     5.61	       
1.7.37	 LTC1266CS	 1C2	  1	 0.3409	 0.3409	     5.61	       
1.7.38	 RECTIFIER	 Q6	  1	 0.07381	 0.07381	     1.21	       
1.7.39	 P CHANNEL JFET	 Q3	  1	 0.3956	 0.3956	     6.51	       
1.7.40	 NPN TRANSISTOR	 Q2	  1	 0.001299	 0.001299	     0.02	       
1.7.41	 NPN TRANSISTOR	 Q1,8	  2	 0.005533	 0.01107	     0.18	       
1.7.42	 FET	 Q5	  1	 0.1846	 0.1846	     3.04	       
1.7.43	 FET	 Q4,7	  2	 0.03357	 0.06713	     1.11	       
1.7.44	 PWB	 PWB	  1	 0.02176	 0.02176	     0.36	       
Applied Values (+Defaults) Report 

  
 HE 104 PWBA <MIL-217F-2 P. stress>  
 Assembly Ref.Des.: A1A1H1,   IC-Analog
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	         
  Type   	                       
 Application(GaAs MMIC)	       # of      
     transist.   	Active
 pins 	          
  Package 	 Years in 
production	        
  Qual  	 Theta 
 jc/ja 	 Power    
 dissipat.	       
 Tc/Ta 	       
  Tj   	
1.7.36	IC1	LTC1159CS-5	 Linear	 ---	  >100 to 300	16	 DIP Nonh	      2.0	 Commerc	   ---	      ---	  32.0	  37.0	              
1.7.37	1C2	LTC1266CS	 Linear	 ---	  >100 to 300	16	 DIP Nonh	      2.0	 Commerc	   ---	      ---	  32.0	  37.0	              
1.7.38	Q6	RECTIFIER	 Linear	 ---	     1 to 100	3	 DIP Nonh	      2.0	 Commerc	   ---	      ---	  32.0	  37.0	              

 Assembly Ref.Des.: A1A1H1,   Resistor
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	       
 Style 	        
  PSR   	        
 Poper  	       
  DT   	                  
       Qual       	
1.7.16	R3-6,..,25	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.17	R13,22	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.18	R15	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.19	R19	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.20	R1,14	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.21	R11,27	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.22	R12,20	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.23	R2,8	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.24	R16,23	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.26	R10	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.27	R26	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.28	R18	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.29	R9	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.30	R7	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        
1.7.31	R23A,23B	RESISTOR	 RM	   0.20	  20.00	   1.0	 M	        

 Assembly Ref.Des.: A1A1H1,   Potentiometer
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	       
 Style 	        
  PSR   	       
  DT   	                  
       Qual       	
1.7.15	R21	RESISTOR	 RV	   0.20	   1.0	 Non-Established	       

 Assembly Ref.Des.: A1A1H1,   Capacitor
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	       
 Style 	             
 Capacitance 	      
 VSR  	 Circuit resist. 
  (CSR & CWR)    	       
  DT   	                  
       Qual       	
1.7.1	C4, C21	CAPACITOR	 CDR	 4.7E-002 uF	 0.20	             ---	   0.0	 M	         
1.7.2	C8,10,19	CAPACITOR	 CDR	    0.100 uF	 0.20	             ---	   0.0	 M	         
1.7.3	C6,17	CAPACITOR	 CDR	 1000.000 pF	 0.20	             ---	   0.0	 M	         
1.7.4	C23	CAPACITOR	 CDR	  100.000 pF	 0.20	             ---	   0.0	 M	         
1.7.5	C9,13,..16	CAPACITOR	 CE	  402.200 uF	 0.20	             ---	   1.0	 Non-Established	         
1.7.6	C5	CAPACITOR	 CDR	  200.000 pF	 0.20	             ---	   0.0	 M	         
1.7.7	C18,24	CAPACITOR	 CDR	    1.000 uF	 0.20	             ---	   0.0	 M	         
1.7.8	C8A-C8D	CAPACITOR	 CE	  402.200 uF	 0.20	             ---	   1.0	 Non-Established	         
1.7.9	C20,22,27	CAPACITOR	 CDR	  330.000 pF	 0.20	             ---	   0.0	 M	         
1.7.10	C25	CAPACITOR	 CWR	    4.700 uF	 0.20	          0.1000	   0.0	 M	         
1.7.11	C1,7,12	CAPACITOR	 CWR	    4.000 uF	 0.20	          0.1000	   0.0	 M	         
1.7.12	C9B,C9C	CAPACITOR	 CE	  402.200 uF	 0.20	             ---	   1.0	 Non-Established	         
1.7.13	C11	CAPACITOR	 CDR	  100.000 pF	 0.20	             ---	   0.0	 M	         
1.7.14	C14	CAPACITOR	 CWR	    1.000 uF	 0.20	          0.1000	   0.0	 M	         
1.7.25	C2,3	CAPACITOR	 CE	  402.200 uF	 0.20	             ---	   1.0	 Non-Established	         

 Assembly Ref.Des.: A1A1H1,   LF Diode
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	             
    Style    	     
 VSR 	                
  Application   	              
 Construction 	  Forward  
 current(A)	         
  Qual   	 Theta 
 jc/ja 	 Power    
 dissipat.	       
 Tc/Ta 	       
  Tj   	
1.7.34	D4,7	DIODE	 DIODE_SI	 0.2	 Voltage Refere	 Non-metallur	       ---	 LOWER	   ---	      ---	  32.0	  33.0	             

 Assembly Ref.Des.: A1A1H1,   LF Transistor
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	             
    Style    	     
 VSR 	                
  Application   	  Power    
  rated    	         
  Qual   	 Theta 
 jc/ja 	 Power    
 dissipat.	       
 Tc/Ta 	       
  Tj   	
1.7.39	Q3	P CHANNEL JFET	 FET_SI_JFET	 ---	 Linear	     1.000	 LOWER	   ---	      ---	  32.0	  33.0	            
1.7.40	Q2	NPN TRANSISTOR	 NPN_SI	 0.0	 Linear	     1.000	 JAN	   ---	      ---	  32.0	  33.0	            
1.7.41	Q1,8	NPN TRANSISTOR	 NPN_GE	 0.2	 Linear	     1.000	 LOWER	   ---	      ---	  32.0	  33.0	            
1.7.42	Q5	FET	 FET_SI_JFET	 ---	 Switching	     1.000	 LOWER	   ---	      ---	  32.0	  33.0	            
1.7.43	Q4,7	FET	 FET_SI_JFET	 ---	 Switching	     1.000	 JANTX	   ---	      ---	  32.0	  33.0	            

 Assembly Ref.Des.: A1A1H1,   Optoelectronic
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	                                   
                Style              	 # of characters 
    (DISPLAY)    	 Logic exists  
 (DISPLAY)     	         
  Qual   	 Theta 
 jc/ja 	 Power    
 dissipat.	       
 Tc/Ta 	       
  Tj   	
1.7.35	LED1-4	LED	 LED DISCRETE	 ---	 ---	 LOWER	   ---	      ---	  32.0	  52.0	           

 Assembly Ref.Des.: A1A1H1,   Inductive
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	                                
         Family type            	       
  DT   	          
   Qual   	
1.7.32	L2	TOR-50	 Coil,Fixed Inductor or Choke	   5.0	 Lower	      
1.7.33	L3	COIL	 Coil,Fixed Inductor or Choke	   5.0	 Lower	      

 Assembly Ref.Des.: A1A1H1,   PWB
                          
 ID                      	           
 Ref.des.  	                               
 PN                            	            
 Technology 	  # of  
 layers 	          
 WAVE(N1) 	          
 HAND(N2) 	          
   Qual   	
1.7.44	PWB	PWB	 Printed wi	 2	 100	 2	 Lower